1. **Introduction**

This is a sample code that demonstrates the function of PWMIO simultaneously. The code is executed on SPI Flash and the unSPIDE tool is needed to download the code to SPI Flash.

1. **Preparation**
   1. Tools:
      1. unSPIDE V3.0.13 or later versions
   2. Hardware requirement
      1. GPL95100UA EMU Board V1.1
      2. ICE ( USB PROBE III )
2. **Run project**

**Step1**

Open project “\PWMIO\PWMIO.spj” by unSPIDE (File->Open Project) and then Rebuild all (Build->Rebuild all)

**Step2**

Connect USB PROBE III to PC and GPL95100UA EMU Board

**Step3**

Download and then free run by “Build/Start Debug/Go” or F5

